Lab 1 – Interface Techniques

Part 2 – change to 19200 baud

SPBRG1 = 520; //19200 baud

SPBRGH1 = 520 >> 8;